#N canvas 156 234 600 488 12;
#X obj 67 124 hilbert~;
#X obj 66 85 osc~ 440;
#X graph graph1 0 -1 882 1 279 209 579 39;
#X array out-left 882 float;
#X array out-right 882 float;
#X pop;
#X obj 67 274 tabwrite~ out-left;
#X obj 118 248 tabwrite~ out-right;
#X msg 137 188 bang \; pd dsp 1;
#X floatatom 66 57;
#X text 71 319 The Hilbert transform (the name is abused here according to computer music tradition) puts out a phase quadrature version of the input signal suitable for signal sideband modulation via complex-mod~.;
#X connect 0 0 3 0;
#X connect 0 1 4 0;
#X connect 1 0 0 0;
#X connect 5 0 3 0;
#X connect 5 0 4 0;
#X connect 6 0 1 0;
